#### TMS Infrastructure
Domain Message Specification

### Messages

Implementations: TMS ITK

| RMIM | Tabular View | Mif | Schema
Send Message Payload (MCCI_MT010101UK12) This message is the outer transport wrapper for all NPfIT domain messages with the exception of specific business response interactions which use an application acknowledgement wrapper. It identifies the sender and recipient of the message and contains the "controlled act" that is being sent. View Examples | View | View | View | View
Application Acknowledgement (MCCI_MT020101UK12) The application acknowledgement wrapper enables a response indicating either successful receipt of the message or that the message has been received containing issues or errors. View Examples | View | View | View | View
Trigger Event Control Act (MCAI_MT040101UK03) This control act is designed for use by all domains. It provides audit functionality by carrying the identity of the person and/or system responsible for initiating the message and enables the optional reporting of detected issues/errors. View Examples | View | View | View | View
Query Acknowledgement Response (QUQI_MT030101UK03) The Query Acknowledgement Response defines the control act used in all query responses. It contains an optional domain response and an option to report issues/errors. View Examples | View | View | View | View
Query Control Act (QUQI_MT050000UK01) The Query Control Act is designed for use by all queries. It provides audit functionality by carrying the identity of the person and/or system responsible for initiating the messages. View Examples | View | View | View | View