#### TMS Infrastructure
Domain Message Specification

### R_AgentNPFITSystemSDSMandated Tabular View

UKCT_RM121000UK01 |
AgentSystemSDS | Identifies a mandatory system which could be software or hardware. Full details of the system are available from SDS.
| Used by:
[1..1] classCode (CS { CNE:AGNT} ){ } Fixed="AGNT" | Indicates that this is an Agent Fixed value: "AGNT"
[1..1] agentSystemSDS (SystemSDS) | A link to the system playing the role.
SystemSDS |
| Used by: AgentSystemSDS
[1..1] classCode (CS { CNE:DEV} ){ } Fixed="DEV" | Indicates that this is a Device. The device represents either a hardware or software system. Fixed value: "DEV"
[1..1] determinerCode (CS { CNE:INSTANCE} ){ } Fixed="INSTANCE" | Indicates that this is a single identifiable Device Fixed value: "INSTANCE"
[1..1] id (II) | An identifier that uniquely identifies the accredited system or workstation id. This is carried in the following way: The root attribute shall contain an OID with the appropriate value the extension attribute shall contain the appropriate identifier The accredited system is represented by the SDS Accredited Application Instance Id held in the SDS directory as the Accredited System Identifier where the value of the OID is 1.2.826.0.1285.0.2.0.107